Written comments

Yes. I generated a wave file with 3 channels with a sampling rate of 8kHz and 16-bits per sample, and the frequency of each channel is 261.1Hz, 440.0Hz, 220.0Hz so that they have different waveforms. I plot the 3 individual channels in the same figure and zoom in with showing the 1 to 64 sample.